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1. Identification
	Product name
	MINERAL ARMOR PROTECTOR RTU

	Other identification
	Use-dilution of MINERAL ARMOR Concentrated Protector. Ready-to-use mixture.

	Recommended use
	Protective floor coating.

	Restrictions on use
	Reserved for industrial and professional use.

	Supplier
	MINERAL ARMOR, 30735 Durand Avenue, Burlington, WI 53105 USA

	Telephone
	+1 414-788-9208

	Email
	SALES@MINERALARMOR.COM

	Emergency telephone
	+1 414-788-9208


ZIP code corrected from 63105 to 53105 (Burlington, Wisconsin). Confirm before distribution.
2. Hazard(s) identification
Classification (OSHA HCS 2012 / HPR)
	Skin corrosion/irritation
	Category 2

	Serious eye damage/eye irritation
	Category 2A

	Acute oral toxicity
	Not classified. Acute Toxicity Category 5 is not adopted under OSHA HCS or WHMIS.


Label elements
	Pictogram
	Exclamation mark

	Signal word
	WARNING

	Hazard statements
	H315 Causes skin irritation.  H319 Causes serious eye irritation.


Precautionary statements
	Prevention
	P264 Wash hands and any exposed skin thoroughly after handling. P280 Wear protective gloves and eye protection/face protection. P102 Keep out of reach of children. P103 Read label before use.

	Response
	P302+P352 IF ON SKIN: Wash with plenty of water. P321 Specific treatment: wash thoroughly with soap and water. P332+P313 If skin irritation occurs: Get medical advice/attention. P362+P364 Take off contaminated clothing and wash it before reuse. P305+P351+P338 IF IN EYES: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing. P337+P313 If eye irritation persists: Get medical advice/attention.

	Storage
	No storage statement is required for this classification. Keep container tightly closed. See Section 7.

	Disposal
	P501 Dispose of contents/container in accordance with local, state, and federal regulations.


Hazards not otherwise classified: None known to the supplier.
Unknown acute toxicity: No ingredient of unknown acute toxicity is present at or above 1%.
3. Composition / information on ingredients
Mixture. Exact concentrations are withheld as a trade secret.
	Ingredient
	Weight %
	CAS No.

	Silicic acid, potassium salt (potassium silicate)
	3 – 8
	Trade Secret

	Potassium methylsiliconate
	0.2 – 1
	Trade Secret

	Water and other non-hazardous components
	Balance
	7732-18-5 (water)


CAS numbers are the published identities for the ingredients named in Section 15. Exact percentages remain a trade secret.
4. First-aid measures
	Eye contact
	Rinse cautiously with potable water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing. If eye irritation persists, get medical advice/attention.

	Skin contact
	Wash with plenty of soap and water. Take off contaminated clothing and wash it before reuse. If skin irritation occurs, get medical advice/attention.

	Inhalation
	Remove person to fresh air and keep comfortable for breathing. Seek medical attention if breathing is difficult.

	Ingestion
	Rinse mouth with water. Do not induce vomiting. Get medical advice/attention if you feel unwell.

	Most important symptoms
	Redness, pain, and irritation of the eyes. Redness and irritation of the skin. Delayed effects are not expected under normal use.

	Notes to physician
	Treat symptomatically. No specific antidote is known.


5. Fire-fighting measures
	Suitable extinguishing media
	Use extinguishing measures appropriate to the surrounding fire. The product is not flammable.

	Unsuitable media
	None known.

	Specific hazards
	Not flammable or combustible. Not an explosion hazard under normal conditions.

	Hazardous combustion products
	Silicon oxides and potassium oxides. Small amounts of carbon oxides may form from the organic siliconate.

	Advice for firefighters
	Wear standard protective equipment and self-contained breathing apparatus if the surrounding fire requires it. Do not breathe fumes. Fire residues and contaminated extinguishing water must be disposed of in accordance with local regulations.


6. Accidental release measures
Personal precautions
Ensure adequate ventilation. Keep unnecessary people away from the spill. Avoid contact with skin, eyes, and clothing, and avoid breathing spray mist. Clean-up should be done by trained personnel. See Sections 7 and 8.
Environmental precautions
Do not allow the product to enter soil, surface water, or groundwater. For large spills, dike the material so runoff does not reach a waterway.
Methods for containment and cleaning up
Stop the leak if it is safe to do so. Contain the spill and collect it with a non-combustible absorbent (sand, earth, diatomaceous earth, or vermiculite). Place in a container for disposal under Section 13. Flush traces with water.
7. Handling and storage
Precautions for safe handling
Avoid contact with eyes, skin, and clothing. Wash thoroughly after handling. Use only in well-ventilated areas. Avoid breathing vapors or spray mist. Remove and wash contaminated clothing and footwear before reuse. Do not eat, drink, or smoke when using this product.
Conditions for safe storage
Store between 5 °C and 40 °C (41 °F to 104 °F). Keep from freezing. Keep the container sealed when not in use. Keep out of reach of children. Incompatible with acids and oxidizing agents.
Specific end use
Protective floor coating. Ready to use; do not dilute further unless directed by product instructions.
8. Exposure controls / personal protection
Occupational exposure limits
No OSHA PEL, ACGIH TLV, or other occupational exposure limit is established for the ingredients in this mixture.
Engineering controls
General dilution ventilation that cycles fresh air through the work area is normally sufficient. Provide an eyewash station where splashing is possible.
Personal protective equipment
	Eye/face
	Wear eye protection or face protection (chemical splash goggles).

	Hands
	Wear protective gloves. Neoprene or rubber gloves are suitable.

	Skin/body
	Long sleeves. An apron is recommended where splashing is likely.

	Respiratory
	Not normally required. If spray mist is generated above comfortable levels, use an appropriate certified respirator.

	Hygiene
	Handle in accordance with good industrial hygiene. Wash face, hands, and any exposed skin after handling.


Environmental exposure controls: No specific control is known beyond preventing release to soil and water.
9. Physical and chemical properties
	Appearance
	Clear liquid
	Odor
	Neutral

	pH
	10.4
	Relative density
	1.000

	Freezing point
	Below 0 °C
	Boiling point
	> 100 °C

	Flash point
	Not applicable
	Flammability
	Not flammable

	Evaporation rate
	No data available
	Vapor pressure
	No data available

	Solubility
	Soluble in water
	Partition coefficient
	No data available

	Auto-ignition temp.
	No data available
	Decomposition temp.
	No data available

	Viscosity
	No data available
	Explosive properties
	Not explosive

	Oxidizing properties
	Not oxidizing
	VOC
	No VOC


10. Stability and reactivity
	Reactivity
	None known under normal conditions.

	Chemical stability
	Stable under normal storage and use.

	Hazardous reactions
	No hazardous reaction expected under normal use.

	Conditions to avoid
	Freezing. Contact with incompatible materials.

	Incompatible materials
	Acids and oxidizing agents.

	Hazardous decomposition
	Silicon oxides and potassium oxides; small amounts of carbon oxides from the methyl siliconate.


11. Toxicological information
Information is for the ready-to-use mixture. Likely routes of exposure: eye contact, skin contact, inhalation of spray mist, ingestion.
	Eyes
	Causes serious eye irritation (Category 2A).

	Skin
	Causes skin irritation (Category 2).

	Ingestion
	Not classified as harmful if swallowed at this use dilution.

	Inhalation
	Not expected to cause injury under normal use. Spray mist may irritate the respiratory tract.

	Sensitization
	Not expected to cause skin or respiratory sensitization.

	Germ cell mutagenicity
	No data indicating mutagenicity. Not expected under normal use.

	Carcinogenicity
	No ingredient is listed by IARC, NTP, or OSHA as a carcinogen at these concentrations.

	Reproductive toxicity
	No data available. Not expected under normal use.

	STOT single / repeated
	Not classified. Chronic effects are not known or expected under normal use.

	Aspiration hazard
	Not applicable. Aqueous liquid.


Numerical toxicity data for the mixture are not available. Classification is based on ingredient data and concentration.
12. Ecological information
	Ecotoxicity
	No data available for the mixture.

	Fish
	No data available.

	Aquatic invertebrates
	No data available.

	Algae
	No data available.

	Persistence / degradability
	Inorganic silicate components do not biodegrade. They are expected to form silica.

	Bioaccumulation
	Not expected. Inorganic salts.

	Mobility in soil
	Soluble in water; may be mobile until it reacts or dries.

	Other effects
	Alkaline product. Do not release to surface water.


13. Disposal considerations
This sheet covers the ready-to-use product.
Do not allow product to enter drains, watercourses, or soil. Recycling is preferred to disposal or incineration. If recycling is not practicable, dispose of in compliance with local regulations at an approved waste facility.
Dispose of unused product and contaminated absorbent as required by local, state, and federal rules. Empty containers should go to an approved waste handler for recycling or disposal. Do not reuse empty containers.
14. Transport information
The shipper is responsible for packaging, labeling, and markings that match the selected mode of transport.
	DOT (US)
	Not regulated

	TDG (Canada)
	Not regulated

	IMDG
	Not regulated. Not a marine pollutant.

	IATA
	Not regulated

	ADR
	Not regulated


15. Regulatory information
United States
TSCA: All components are listed on the TSCA inventory (potassium silicate and potassium methylsiliconate are listed under TSCA Section 8(b)).
SARA 302 extremely hazardous substances: None. SARA 304: None. SARA 313 toxic chemicals: None.
CERCLA hazardous substances: None. Clean Air Act listed substances: None. Clean Water Act listed substances: None.
California Proposition 65: No substances listed. Massachusetts, Pennsylvania, and New Jersey Right-to-Know: no substances listed for this mixture.
Canada
DSL: All substances are listed. NDSL: none. NPRI: no substances listed.
This product has been classified in accordance with the hazard criteria of the Hazardous Products Regulations (HPR), and this SDS contains all information required by the HPR.
Other inventories
Listed or compliant, where checked by the supplier: Korea ECL, Japan ENCS, Australia AIIC, China IECSC, Philippines PICCS, EU REACH (registration obligations for import into or manufacture in the EEA rest with the importer or manufacturer).
HMIS ratings (informational)
	Health
	2

	Flammability
	0

	Physical hazard
	0


0 = minimal, 1 = slight, 2 = moderate, 3 = serious, 4 = severe. These ratings are not part of the OSHA or HPR label.
16. Other information
	Issue date
	08/30/2026

	Revision date
	10/01/2026

	Version
	2.01

	Prepared by
	MINERAL ARMOR Regulatory Affairs

	Revision summary
	Editorial cleanup. Sections placed in 1–16 order. Spelling and units corrected. Hazard statements and precautionary statements aligned to Skin Irritation Category 2 and Eye Irritation Category 2A. Acute Toxicity Category 5 removed (not adopted by OSHA or WHMIS). Burlington ZIP corrected to 53105. Published CAS numbers added; exact percentages remain a trade secret. Disposal language no longer refers to a further 1:4 dilution.


The information in this safety data sheet is based on the supplier’s knowledge at the date of publication. It is intended to describe the product for health, safety, and environmental purposes and is not a warranty of product properties or fitness for a particular use.
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